



To get LG02 working with TTN



Have to place in nodes (RAMD21) Single to transmit/RX on single channel











<<< THIS IS IMPORTANT BIT >>>

